<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="71.374" x2="0" y2="4.826" width="0" layer="20"/>
<wire x1="49.53" y1="4.826" x2="49.53" y2="71.374" width="0" layer="20"/>
<wire x1="48.26" y1="72.644" x2="1.27" y2="72.644" width="0" layer="20"/>
<text>7mm for IDC</text>
<text>.01" for IDC Clearance</text>
<text>7.5-8mm clearance under board</text>
<text>2.4" to frame (2.43" actual)</text>
<text>.02" for IDC
inc protrusion</text>
<text>GND</text>
<text>RST</text>
<text>TMS</text>
<text>TDO</text>
<text>TDI</text>
<text>TCLK</text>
<text>RX</text>
<text>TX</text>
<text>3.3V</text>
<text>VUSB</text>
<text>SCL</text>
<text>SDA</text>
<text>+5V</text>
<text>GND</text>
<wire x1="1.27" y1="3.556" x2="48.26" y2="3.556" width="0" layer="20"/>
<wire x1="0" y1="71.374" x2="1.27" y2="72.644" width="0" layer="20" curve="-90"/>
<wire x1="48.26" y1="72.644" x2="49.53" y2="71.374" width="0" layer="20" curve="-90"/>
<wire x1="49.53" y1="4.826" x2="48.26" y2="3.556" width="0" layer="20" curve="-90"/>
<wire x1="1.27" y1="3.556" x2="0" y2="4.826" width="0" layer="20" curve="-90"/>
<text>BLK</text>
<text>RED</text>
<text>WHT</text>
<text>RED WIRE</text>
<text>POWER</text>
<text>USB</text>
<text>AUDIO
INPUT</text>
<text>PANEL
DATA</text>
<text>IR</text>
<text>SmartMatrix</text>
<text>V1</text>
<text>2015-03-30</text>
<text>SmartMatrix</text>
<text>V1</text>
<text>pixl.mx/smbrd01</text>
<text>J7</text>
<text>SmartMatrix
2015 Pixelmatix CC-BY-SA
"Hacker Port" and basic microcontroller
circuit modified from original by scanlime</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="MICROSD">
</package>
<package name="DCJACK_2MM_PTH">
<description>DJ Jack 2.0mm PTH Right-Angle</description>
</package>
<package name="XTAL3215">
</package>
</packages>
</library>
<library name="eclibrary">
<packages>
<package name="2X08-NOA">
</package>
<package name="BU2032-SM">
</package>
<package name="TSSOP-20">
</package>
<package name="4,1-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 4.1 mm, round</description>
</package>
<package name="SOD123">
<description>&lt;b&gt;Diode&lt;/b&gt;</description>
</package>
<package name="LED-REARENTRY">
</package>
<package name="MK20DX256VLH7">
</package>
<package name="1X03-SMD/90-NOA">
</package>
<package name="PIXELMATIX-LOGO-SMALL-IMPORT">
</package>
</packages>
</library>
<library name="scanlime">
<description>Personal parts library of Micah Elizabeth Scott.</description>
<packages>
<package name="TSX-3225">
<description>&lt;b&gt;&lt;b&gt;MHz range crystal unit&lt;/b&gt;

&lt;p&gt;Digi-Key: &lt;a href="http://www.digikey.com/product-detail/en/TSX-3225%2016.0000MF18X-AC3/SER3636CT-ND/1825448"&gt;SER3636CT-ND&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="0805">
<description>0805 (2012 Metric)</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP18SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Teensy_3_Series_Chip_v1.0">
<packages>
<package name="QFP50P900X900X160-48N">
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AUDIO-JACK">
</package>
<package name="USB-B-PTH">
<description>&lt;b&gt;USB Series B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="msgeq7">
<packages>
<package name="SOIC8">
</package>
</packages>
</library>
<library name="microbuilder">
<description>&lt;h2&gt;&lt;b&gt;microBuilder.eu&lt;/b&gt; Eagle Footprint Library&lt;/h2&gt;

&lt;p&gt;Footprints for common components used in our projects and products.  This is the same library that we use internally, and it is regularly updated.  The newest version can always be found at &lt;b&gt;www.microBuilder.eu&lt;/b&gt;.  If you find this library useful, please feel free to purchase something from our online store. Please also note that all holes are optimised for metric drill bits!&lt;/p&gt;

&lt;h3&gt;Obligatory Warning&lt;/h3&gt;
&lt;p&gt;While it probably goes without saying, there are no guarantees that the footprints or schematic symbols in this library are flawless, and we make no promises of fitness for production, prototyping or any other purpose. These libraries are provided for information puposes only, and are used at your own discretion.  While we make every effort to produce accurate footprints, and many of the items found in this library have be proven in production, we can't make any promises of suitability for a specific purpose. If you do find any errors, though, please feel free to contact us at www.microbuilder.eu to let us know about it so that we can update the library accordingly!&lt;/p&gt;

&lt;h3&gt;License&lt;/h3&gt;
&lt;p&gt;This work is placed in the public domain, and may be freely used for commercial and non-commercial work with the following conditions:&lt;/p&gt;
&lt;p&gt;THIS SOFTWARE IS PROVIDED ''AS IS'' AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED.  IN NO EVENT SHALL THE INSTITUTE OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING,  BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
&lt;/p&gt;</description>
<packages>
<package name="FIDUCIAL_1MM">
</package>
</packages>
</library>
<library name="ohw-logo">
<packages>
<package name="OSHW_FILLX70_NOTEXT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="Y1" library="scanlime" package="TSX-3225" value="16 MHz">
<attribute name="NAME"/>
<attribute name="PARTNO" value="TSX-3225 16.0000MF09Z-AC3"/>
</element>
<element name="C1" library="scanlime" package="0805" value="2.2uF">
<attribute name="NAME"/>
<attribute name="PARTNO" value="CAP CER 2.2UF 10V 10% X7R 0805"/>
</element>
<element name="C2" library="scanlime" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PARTNO" value="CAP CER 0.1UF 10V 10% X7R 0805"/>
</element>
<element name="C3" library="scanlime" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PARTNO" value="CAP CER 0.1UF 10V 10% X7R 0805"/>
</element>
<element name="C4" library="scanlime" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PARTNO" value="CAP CER 0.1UF 10V 10% X7R 0805"/>
</element>
<element name="C5" library="scanlime" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="PARTNO" value="CAP CER 10UF 10V 10% X5R 0805"/>
</element>
<element name="C6" library="scanlime" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PARTNO" value="CAP CER 0.1UF 10V 10% X7R 0805"/>
</element>
<element name="FB2" library="scanlime" package="0805" value="FB0805/NO-OUTLINE">
<attribute name="NAME"/>
<attribute name="PARTNO" value="RES SMD 0.0 OHM JUMPER 1/8W 0805"/>
<attribute name="DNP" value="T"/>
</element>
<element name="R3" library="scanlime" package="0805" value="33">
<attribute name="NAME"/>
<attribute name="PARTNO" value="RES 33 OHM 1/8W 5% 0805 SMD"/>
</element>
<element name="R4" library="scanlime" package="0805" value="33">
<attribute name="NAME"/>
<attribute name="PARTNO" value="RES 33 OHM 1/8W 5% 0805 SMD"/>
</element>
<element name="RESET" library="testpad" package="TP18SQ" value="TPTP18SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="PTA3" library="testpad" package="TP18SQ" value="TPTP18SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="PTA2" library="testpad" package="TP18SQ" value="TPTP18SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="PTA1" library="testpad" package="TP18SQ" value="TPTP18SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="PTA0" library="testpad" package="TP18SQ" value="TPTP18SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="J6" library="adafruit" package="MICROSD" value="MICROSD">
<attribute name="NAME"/>
<attribute name="PARTNO" value="101-00660-68-6"/>
</element>
<element name="S4" library="SparkFun" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="DNP" value="T"/>
</element>
<element name="J4" library="eclibrary" package="2X08-NOA" value="CON_HEADER_2X08NOA">
<attribute name="NAME"/>
<attribute name="PARTNO" value="11149"/>
</element>
<element name="IC5" library="Teensy_3_Series_Chip_v1.0" package="QFP50P900X900X160-48N" value="MINI54TANDEFAULT">
<attribute name="NAME"/>
<attribute name="DNP" value="T"/>
</element>
<element name="C9" library="scanlime" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PARTNO" value="CAP CER 0.1UF 10V 10% X7R 0805"/>
</element>
<element name="C10" library="scanlime" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PARTNO" value="CAP CER 0.1UF 10V 10% X7R 0805"/>
</element>
<element name="C11" library="scanlime" package="0805" value="1.0uF">
<attribute name="NAME"/>
<attribute name="DNP" value="T"/>
<attribute name="PARTNO" value="CAP CER 1UF 10V X7R 0805"/>
</element>
<element name="R8" library="scanlime" package="0805" value="4.7k">
<attribute name="NAME"/>
<attribute name="PARTNO" value="RES SMD 4.7K OHM 5% 1/8W 0805"/>
</element>
<element name="J3" library="SparkFun" package="AUDIO-JACK" value="AUDIO-JACK2PTH">
<attribute name="PARTNO" value="SJ1-3553NG"/>
</element>
<element name="J1" library="adafruit" package="DCJACK_2MM_PTH" value="">
<attribute name="VALUE"/>
<attribute name="PARTNO" value="PJ-002AH"/>
</element>
<element name="J2" library="SparkFun" package="USB-B-PTH" value="USB+SHIELD">
<attribute name="PARTNO" value="E8144-B02022-L"/>
</element>
<element name="S3" library="SparkFun" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="DNP" value="T"/>
</element>
<element name="S2" library="SparkFun" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="DNP" value="T"/>
</element>
<element name="IC2" library="msgeq7" package="SOIC8" value="MSGEQ7SOIC">
<attribute name="NAME"/>
<attribute name="PARTNO" value="MSGEQ7N"/>
</element>
<element name="S1" library="SparkFun" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="DNP" value="T"/>
</element>
<element name="J7" library="eclibrary" package="BU2032-SM" value="BATTERY">
<attribute name="PARTNO" value="05581"/>
</element>
<element name="C12" library="scanlime" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PARTNO" value="CAP CER 0.1UF 10V 10% X7R 0805"/>
</element>
<element name="C13" library="scanlime" package="0805" value="0.01uF">
<attribute name="NAME"/>
<attribute name="PARTNO" value="CAP CER 10000PF 50V 10% X7R 0805"/>
</element>
<element name="R1" library="scanlime" package="0805" value="22k">
<attribute name="NAME"/>
<attribute name="PARTNO" value="RES SMD 22K OHM 5% 1/8W 0805"/>
</element>
<element name="R2" library="scanlime" package="0805" value="22k">
<attribute name="NAME"/>
<attribute name="PARTNO" value="RES SMD 22K OHM 5% 1/8W 0805"/>
</element>
<element name="C14" library="scanlime" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PARTNO" value="CAP CER 0.1UF 10V 10% X7R 0805"/>
</element>
<element name="C15" library="scanlime" package="0805" value="33pF">
<attribute name="NAME"/>
<attribute name="PARTNO" value="CAP CER 33PF 50V 5% NP0 0805"/>
</element>
<element name="R5" library="scanlime" package="0805" value="200k">
<attribute name="NAME"/>
<attribute name="PARTNO" value="RES SMD 200K OHM 5% 1/8W 0805"/>
</element>
<element name="R7" library="scanlime" package="0805" value="4.7k">
<attribute name="NAME"/>
<attribute name="PARTNO" value="RES SMD 4.7K OHM 5% 1/8W 0805"/>
</element>
<element name="R6" library="scanlime" package="0805" value="4.7k">
<attribute name="NAME"/>
<attribute name="PARTNO" value="RES SMD 4.7K OHM 5% 1/8W 0805"/>
</element>
<element name="PTE1" library="testpad" package="TP18SQ" value="TPTP18SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="PTE0" library="testpad" package="TP18SQ" value="TPTP18SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="VUSB" library="testpad" package="TP18SQ" value="TPTP18SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="GND" library="testpad" package="TP18SQ" value="TPTP18SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="3.3V" library="testpad" package="TP18SQ" value="TPTP18SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="FID1" library="microbuilder" package="FIDUCIAL_1MM" value="FIDUCIAL&quot;&quot;">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="FID2" library="microbuilder" package="FIDUCIAL_1MM" value="FIDUCIAL&quot;&quot;">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="FID3" library="microbuilder" package="FIDUCIAL_1MM" value="FIDUCIAL&quot;&quot;">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="C16" library="scanlime" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PARTNO" value="CAP CER 0.1UF 10V 10% X7R 0805"/>
</element>
<element name="C8" library="scanlime" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PARTNO" value="CAP CER 0.1UF 10V 10% X7R 0805"/>
</element>
<element name="IC4" library="eclibrary" package="TSSOP-20" value="74245PW">
<attribute name="NAME"/>
<attribute name="PARTNO" value="SN74AHCT245PWR"/>
</element>
<element name="IC3" library="eclibrary" package="TSSOP-20" value="74245PW">
<attribute name="NAME"/>
<attribute name="PARTNO" value="SN74AHCT245PWR"/>
</element>
<element name="Y2" library="adafruit" package="XTAL3215" value="32.768kHz">
<attribute name="NAME"/>
<attribute name="PARTNO" value="9HT10-32.768KDZF-T"/>
</element>
<element name="PTB1" library="testpad" package="TP18SQ" value="TPTP18SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="PTB0" library="testpad" package="TP18SQ" value="TPTP18SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="FB1" library="scanlime" package="0805" value="FB0805/NO-OUTLINE">
<attribute name="NAME"/>
<attribute name="PARTNO" value="RES SMD 0.0 OHM JUMPER 1/8W 0805"/>
<attribute name="DNP" value="T"/>
</element>
<element name="C7" library="scanlime" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PARTNO" value="CAP CER 0.1UF 10V 10% X7R 0805"/>
</element>
<element name="FB3" library="scanlime" package="0805" value="FB0805/NO-OUTLINE">
<attribute name="NAME"/>
<attribute name="PARTNO" value="RES SMD 0.0 OHM JUMPER 1/8W 0805"/>
<attribute name="DNP" value="T"/>
</element>
<element name="VCCMOUNT" library="eclibrary" package="4,1-PAD" value="MOUNT-PAD-ROUND4.1">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="GNDMOUNT" library="eclibrary" package="4,1-PAD" value="MOUNT-PAD-ROUND4.1">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="D3" library="eclibrary" package="SOD123" value="MBR0520LT">
<attribute name="NAME"/>
<attribute name="PARTNO" value="MBR0560-TP"/>
</element>
<element name="D4" library="eclibrary" package="SOD123" value="MBR0520LT">
<attribute name="NAME"/>
<attribute name="PARTNO" value="MBR0560-TP"/>
</element>
<element name="D2" library="eclibrary" package="SOD123" value="MBR0520LT">
<attribute name="NAME"/>
<attribute name="PARTNO" value="MBR0560-TP"/>
</element>
<element name="D1" library="eclibrary" package="SOD123" value="MBR0520LT">
<attribute name="NAME"/>
<attribute name="PARTNO" value="MBR0560-TP"/>
</element>
<element name="D5" library="eclibrary" package="LED-REARENTRY" value="LED1206-REAR">
<attribute name="NAME"/>
<attribute name="PARTNO" value="APTR3216YC"/>
</element>
<element name="R9" library="scanlime" package="0805" value="330">
<attribute name="PARTNO" value="RES SMD 330 OHM 5% 1/8W 0805"/>
<attribute name="NAME"/>
</element>
<element name="D6" library="eclibrary" package="LED-REARENTRY" value="LED1206-REAR">
<attribute name="NAME"/>
<attribute name="DNP" value="T"/>
</element>
<element name="IC1" library="eclibrary" package="MK20DX256VLH7" value="MK20DX256VLH7">
<attribute name="NAME"/>
<attribute name="PARTNO" value="MK20DX256VLH7"/>
</element>
<element name="J5" library="eclibrary" package="1X03-SMD/90-NOA" value="CON_HEADER_1X03SMD/90-NOA">
<attribute name="PARTNO" value="11182"/>
<attribute name="NAME"/>
</element>
<element name="U$2" library="eclibrary" package="PIXELMATIX-LOGO-SMALL-IMPORT" value=""/>
<element name="U$1" library="ohw-logo" package="OSHW_FILLX70_NOTEXT" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="FB2" pad="2"/>
<contactref element="J4" pad="4"/>
<contactref element="J4" pad="8"/>
<contactref element="J4" pad="16"/>
<contactref element="C10" pad="2"/>
<contactref element="IC5" pad="5"/>
<contactref element="IC5" pad="17"/>
<contactref element="IC5" pad="25"/>
<contactref element="IC5" pad="47"/>
<contactref element="C11" pad="2"/>
<contactref element="J6" pad="6"/>
<contactref element="J6" pad="MT2"/>
<contactref element="J6" pad="MT1"/>
<contactref element="J1" pad="GND"/>
<contactref element="J1" pad="GND"/>
<contactref element="J2" pad="S1"/>
<contactref element="J2" pad="S2"/>
<contactref element="J7" pad="-"/>
<contactref element="R6" pad="1"/>
<contactref element="S1" pad="1"/>
<contactref element="S2" pad="1"/>
<contactref element="S3" pad="1"/>
<contactref element="GND" pad="TP"/>
<contactref element="C16" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="IC4" pad="10"/>
<contactref element="IC3" pad="10"/>
<contactref element="IC4" pad="10"/>
<contactref element="IC3" pad="10"/>
<contactref element="C9" pad="2"/>
<contactref element="IC4" pad="19"/>
<contactref element="IC3" pad="19"/>
<contactref element="IC3" pad="4"/>
<contactref element="IC3" pad="3"/>
<contactref element="C7" pad="2"/>
<contactref element="FB3" pad="1"/>
<contactref element="GNDMOUNT" pad="B4,1"/>
<contactref element="S4" pad="3"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="47"/>
<contactref element="IC1" pad="15"/>
<contactref element="IC1" pad="16"/>
<contactref element="D5" pad="-"/>
<contactref element="D6" pad="-"/>
<contactref element="IC3" pad="2"/>
<contactref element="J5" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="Y1" pad="1"/>
<contactref element="IC1" pad="33"/>
</signal>
<signal name="+5V">
<contactref element="C6" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="VUSB" pad="TP"/>
<contactref element="IC4" pad="20"/>
<contactref element="IC4" pad="1"/>
<contactref element="IC3" pad="1"/>
<contactref element="IC3" pad="20"/>
<contactref element="C8" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="R8" pad="2"/>
<contactref element="D3" pad="C"/>
<contactref element="D4" pad="C"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="+3V3">
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="IC5" pad="43"/>
<contactref element="IC5" pad="42"/>
<contactref element="J6" pad="4"/>
<contactref element="IC2" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="3.3V" pad="TP"/>
<contactref element="C9" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="D2" pad="A"/>
<contactref element="IC1" pad="7"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="30"/>
<contactref element="IC1" pad="48"/>
<contactref element="IC1" pad="13"/>
<contactref element="IC1" pad="14"/>
<contactref element="J5" pad="3"/>
</signal>
<signal name="PANEL_R1">
<contactref element="J4" pad="1"/>
<contactref element="IC4" pad="11"/>
</signal>
<signal name="PANEL_B1">
<contactref element="J4" pad="3"/>
<contactref element="IC4" pad="15"/>
</signal>
<signal name="PANEL_R2">
<contactref element="J4" pad="5"/>
<contactref element="IC4" pad="17"/>
</signal>
<signal name="PANEL_B2">
<contactref element="J4" pad="7"/>
<contactref element="IC4" pad="16"/>
</signal>
<signal name="PANEL_ADX0">
<contactref element="J4" pad="9"/>
<contactref element="IC3" pad="12"/>
</signal>
<signal name="PANEL_ADX2">
<contactref element="J4" pad="11"/>
<contactref element="IC3" pad="11"/>
</signal>
<signal name="PANEL_G1">
<contactref element="J4" pad="2"/>
<contactref element="IC4" pad="18"/>
</signal>
<signal name="PANEL_G2">
<contactref element="J4" pad="6"/>
<contactref element="IC4" pad="13"/>
</signal>
<signal name="PANEL_ADX1">
<contactref element="J4" pad="10"/>
<contactref element="IC3" pad="14"/>
</signal>
<signal name="PANEL_LATCH">
<contactref element="J4" pad="14"/>
<contactref element="IC4" pad="14"/>
</signal>
<signal name="PANEL_CLK">
<contactref element="J4" pad="13"/>
<contactref element="IC4" pad="12"/>
</signal>
<signal name="PANEL_ADX3">
<contactref element="J4" pad="12"/>
<contactref element="IC3" pad="13"/>
</signal>
<signal name="N$12">
<contactref element="R4" pad="2"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="Y1" pad="3"/>
<contactref element="IC1" pad="32"/>
</signal>
<signal name="PTA2">
<contactref element="PTA2" pad="TP"/>
<contactref element="IC5" pad="37"/>
<contactref element="IC1" pad="24"/>
</signal>
<signal name="PTA0">
<contactref element="PTA0" pad="TP"/>
<contactref element="IC5" pad="32"/>
<contactref element="IC1" pad="22"/>
</signal>
<signal name="PTA3">
<contactref element="PTA3" pad="TP"/>
<contactref element="IC5" pad="34"/>
<contactref element="IC5" pad="33"/>
<contactref element="IC1" pad="25"/>
</signal>
<signal name="PTA1">
<contactref element="PTA1" pad="TP"/>
<contactref element="IC5" pad="38"/>
<contactref element="IC1" pad="23"/>
</signal>
<signal name="N$11">
<contactref element="R3" pad="2"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="N$15">
<contactref element="Y2" pad="P$1"/>
<contactref element="IC1" pad="19"/>
</signal>
<signal name="N$16">
<contactref element="Y2" pad="P$2"/>
<contactref element="IC1" pad="20"/>
</signal>
<signal name="VBAT">
<contactref element="C10" pad="1"/>
<contactref element="D2" pad="C"/>
<contactref element="D1" pad="C"/>
<contactref element="IC1" pad="21"/>
</signal>
<signal name="RESET">
<contactref element="IC5" pad="8"/>
<contactref element="RESET" pad="TP"/>
<contactref element="IC1" pad="34"/>
</signal>
<signal name="N$19">
<contactref element="IC5" pad="18"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="VEXT">
<contactref element="J1" pad="PWR"/>
<contactref element="R7" pad="2"/>
<contactref element="VCCMOUNT" pad="B4,1"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="VCOIN">
<contactref element="J7" pad="+"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="SPI_MISO">
<contactref element="J6" pad="7"/>
<contactref element="IC1" pad="52"/>
</signal>
<signal name="SPI_MOSI">
<contactref element="J6" pad="3"/>
<contactref element="IC1" pad="51"/>
</signal>
<signal name="24/BUTTON">
<contactref element="IC5" pad="20"/>
<contactref element="S4" pad="1"/>
<contactref element="IC1" pad="41"/>
</signal>
<signal name="N$9">
<contactref element="R4" pad="1"/>
<contactref element="J2" pad="D+"/>
</signal>
<signal name="N$10">
<contactref element="R3" pad="1"/>
<contactref element="J2" pad="D-"/>
</signal>
<signal name="GNDBREAK">
<contactref element="J1" pad="GNDBREAK"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="C13" pad="2"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="TIP">
<contactref element="R2" pad="1"/>
<contactref element="J3" pad="TIP"/>
</signal>
<signal name="RING">
<contactref element="R1" pad="1"/>
<contactref element="J3" pad="RING"/>
</signal>
<signal name="EQ_STB">
<contactref element="IC2" pad="4"/>
<contactref element="IC1" pad="40"/>
</signal>
<signal name="EQ_RST">
<contactref element="IC2" pad="7"/>
<contactref element="IC1" pad="39"/>
</signal>
<signal name="EQ_OUT">
<contactref element="IC2" pad="3"/>
<contactref element="IC1" pad="18"/>
</signal>
<signal name="N$18">
<contactref element="IC2" pad="8"/>
<contactref element="C15" pad="1"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="IC2" pad="6"/>
<contactref element="C14" pad="1"/>
</signal>
<signal name="18/IR">
<contactref element="IC5" pad="9"/>
<contactref element="IC1" pad="38"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="SPI_CS">
<contactref element="J6" pad="2"/>
<contactref element="IC1" pad="43"/>
</signal>
<signal name="SPI_SCK">
<contactref element="J6" pad="5"/>
<contactref element="IC1" pad="50"/>
</signal>
<signal name="VEXT_SENSE">
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="VUSB">
<contactref element="FB1" pad="2"/>
<contactref element="D4" pad="A"/>
<contactref element="FB1" pad="1"/>
<contactref element="J2" pad="VBUS"/>
</signal>
<signal name="19/MINI54">
<contactref element="IC5" pad="10"/>
<contactref element="IC1" pad="37"/>
</signal>
<signal name="BUFFER_R1">
<contactref element="IC4" pad="9"/>
<contactref element="IC1" pad="57"/>
</signal>
<signal name="BUFFER_B1">
<contactref element="IC4" pad="5"/>
<contactref element="IC1" pad="61"/>
</signal>
<signal name="BUFFER_R2">
<contactref element="IC4" pad="3"/>
<contactref element="IC1" pad="63"/>
</signal>
<signal name="BUFFER_B2">
<contactref element="IC4" pad="4"/>
<contactref element="IC1" pad="62"/>
</signal>
<signal name="BUFFER_ADX0">
<contactref element="IC3" pad="8"/>
<contactref element="IC1" pad="46"/>
</signal>
<signal name="BUFFER_ADX2">
<contactref element="IC3" pad="9"/>
<contactref element="IC1" pad="44"/>
</signal>
<signal name="BUFFER_CLK">
<contactref element="IC4" pad="8"/>
<contactref element="IC1" pad="58"/>
</signal>
<signal name="BUFFER_OE">
<contactref element="R8" pad="1"/>
<contactref element="IC3" pad="5"/>
<contactref element="IC1" pad="29"/>
</signal>
<signal name="BUFFER_G1">
<contactref element="IC4" pad="2"/>
<contactref element="IC1" pad="64"/>
</signal>
<signal name="BUFFER_G2">
<contactref element="IC4" pad="7"/>
<contactref element="IC1" pad="59"/>
</signal>
<signal name="BUFFER_ADX1">
<contactref element="IC3" pad="6"/>
<contactref element="IC1" pad="49"/>
</signal>
<signal name="BUFFER_ADX3">
<contactref element="IC3" pad="7"/>
<contactref element="IC1" pad="45"/>
</signal>
<signal name="BUFFER_LATCH">
<contactref element="IC4" pad="6"/>
<contactref element="IC1" pad="60"/>
<contactref element="IC1" pad="28"/>
</signal>
<signal name="PANEL_OE">
<contactref element="J4" pad="15"/>
<contactref element="IC3" pad="15"/>
</signal>
<signal name="UART1_TX">
<contactref element="PTE0" pad="TP"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="UART1_RX">
<contactref element="PTE1" pad="TP"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="SWITCH1">
<contactref element="S1" pad="3"/>
<contactref element="IC1" pad="56"/>
</signal>
<signal name="SWITCH2">
<contactref element="S2" pad="3"/>
<contactref element="IC1" pad="55"/>
</signal>
<signal name="SWITCH3">
<contactref element="S3" pad="3"/>
<contactref element="IC1" pad="53"/>
</signal>
<signal name="17_SDA">
<contactref element="PTB1" pad="TP"/>
<contactref element="IC1" pad="36"/>
</signal>
<signal name="16_SCL">
<contactref element="PTB0" pad="TP"/>
<contactref element="IC1" pad="35"/>
</signal>
<signal name="AGND">
<contactref element="J3" pad="SLEEVE"/>
<contactref element="C12" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="IC2" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="FB3" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="D5" pad="+"/>
<contactref element="D6" pad="+"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="STATUS_LED">
<contactref element="IC1" pad="27"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="XTAL_GND">
<contactref element="Y1" pad="2"/>
<contactref element="Y1" pad="4"/>
<contactref element="IC1" pad="31"/>
</signal>
<signal name="N$17">
</signal>
<signal name="N$3">
<contactref element="J2" pad="GND"/>
<contactref element="FB2" pad="1"/>
</signal>
<signal name="N$7">
</signal>
</signals>
</board>
</drawing>
</eagle>
